CB 80 channel for 92R W1-Band 470-500

Hardware Code:950292780050                              Software Code: 110200200000000

9 - Mobile.                                             1 - Continuous Channel display.
2 - Medium Simplex.                                     1 - Variable Mute, with defeat.
7 - W1-Band 470-500.                                    0 - No economiser.
8 - Remote Control 12.5 Khz chl Space.                  2 - 3 Minute TX Timer.
0 - Standard Mechanical.                                0 - No Tx inhibit.
0 - No signalling Hardware.                             0 - Tx power: 25W.
5 - No selcall with I/O Expansion Kit.                  2 - Scan: occupied, pre-pro blocks.
0 - Standard Version.                                   0 - No voting.
                                                        0 - No CTCSS.                   
                                                        0 - No tone Period.
                                                        0 - Simplex Mode.
                                                        00 - Selcall Encode.
                                                        00 - Selcall Decode.

=============================================================================================

This file is for a fm92R "Remote" W1-Band 470-500

channels 93

Channel 1 to 80 as per CB listing
Channel 1 to 8 are duplex
Channel 41 to 48 are duplex
Channels 81 to 88 simplex for channels 1 to 8
Channels 91 to 98 simplex for channels 41 to 48

Scan
-----

Scan group 1: 1,2,3,4,5,6,7,8,9,10
Scan group 2: 11,12,13,14,15,16,17,18,39,40


File made buy BuNtEr
7/5/2020 @ 6:07PM

